ATMEL: wdt_drv.c File Reference

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# wdt_drv.c File Reference

`#include "config.h"`
`#include "wdt_drv.h"`

Include dependency graph for wdt_drv.c:

Go to the source code of this file.

## Defines

#define | Wdt_reset_instruction() __watchdog_reset()

## Functions

void | wdtdrv_disable (void)
| This functions stops the hardware watchdog timer.
void | wdtdrv_enable (U8 timeout)
| This functions activates the hardware watchdog timer System Reset Mode only.
void | wdtdrv_interrupt_enable (U8 timeout)
| This functions activates the hardware watchdog timer Interrupt Mode only.
void | wdtdrv_interrupt_reset_enable (U8 timeout)
| This functions activates the hardware watchdog timer Interrupt & System Reset Mode.

## Detailed Description

This file contains the Watchdog low level driver definition - Compiler: IAR EWAVR and GNU GCC for AVR

- Supported devices: AT90USB162, AT90USB82
  Author:
    Atmel Corporation: http://www.atmel.com
    Support and FAQ: http://support.atmel.no/

Definition in file wdt_drv.c.

## Define Documentation

#define Wdt_reset_instruction | ( |  | ) | __watchdog_reset()

Definition at line 51 of file wdt_drv.c.

Referenced by wdtdrv_disable(), wdtdrv_enable(), wdtdrv_interrupt_enable(), and wdtdrv_interrupt_reset_enable().