ATMEL: Fs_index Struct Reference

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Alphabetical List
- Data Structures
- Data Fields

# Fs_index Struct Reference

`#include <fs_com.h>`

## Data Fields

U8 | u8_lun
| number of the logical driver
U8 | u8_partition
| number of the partition - 1 (0 or 1) (if FS_MULTI_PARTITION == ENABLED)
U32 | u32_cluster_sel_dir
| first cluster of the directory corresponding at the selected file
U16 | u16_entry_pos_sel_file
| entry offset of selected file in selected directory (unit = FS_SIZE_FILE_ENTRY)

## Detailed Description

Definition at line 176 of file fs_com.h.

## Field Documentation

U8 Fs_index::u8_lun

number of the logical driver

Definition at line 177 of file fs_com.h.

Referenced by nav_getindex().

U8 Fs_index::u8_partition

number of the partition - 1 (0 or 1) (if FS_MULTI_PARTITION == ENABLED)

Definition at line 179 of file fs_com.h.

Referenced by nav_getindex().

U32 Fs_index::u32_cluster_sel_dir

first cluster of the directory corresponding at the selected file

Definition at line 181 of file fs_com.h.

Referenced by nav_getindex().

U16 Fs_index::u16_entry_pos_sel_file

entry offset of selected file in selected directory (unit = FS_SIZE_FILE_ENTRY)

Definition at line 182 of file fs_com.h.

Referenced by nav_getindex().

The documentation for this struct was generated from the following file:

- fs_com.h