ATMEL: ADC Start Normal Conversion

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# ADC Start Normal Conversion
[ADC Start Conversion]

Start the conversion in normal mode. More...

## Defines

#define | Start_conv() (ADCSRA |= (1<<ADSC) )
#define | Start_conv_channel(channel) (Select_adc_channel(channel), Start_conv() )
#define | Start_amplified_conv() (ADCSRB |= (1<<ADASCR) )
#define | Stop_amplified_conv() (ADCSRB &= ~(1<<ADASCR) )
#define | Start_amplified_conv_channel(channel) (Select_adc_channel(channel), Start_amplified_conv() )

## Detailed Description

Start the conversion in normal mode.

## Define Documentation

#define Start_conv | ( |  | ) | (ADCSRA |= (1<<ADSC) )

Definition at line 120 of file adc_drv.h.

#define Start_conv_channel | ( | channel |  | ) | (Select_adc_channel(channel), Start_conv() )

Definition at line 121 of file adc_drv.h.

#define Start_amplified_conv | ( |  | ) | (ADCSRB |= (1<<ADASCR) )

Definition at line 122 of file adc_drv.h.

#define Stop_amplified_conv | ( |  | ) | (ADCSRB &= ~(1<<ADASCR) )

Definition at line 123 of file adc_drv.h.

#define Start_amplified_conv_channel | ( | channel |  | ) | (Select_adc_channel(channel), Start_amplified_conv() )

Definition at line 124 of file adc_drv.h.