ATMEL: ADC High Speed Mode Configuration

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# ADC High Speed Mode Configuration
[ADC Macros]

Set the high spped mode in case ADC frequency is higher than 200KHz. More...

## Defines

#define | Enable_adc_high_speed_mode() (ADCSRB |= (1<<ADHSM))
#define | Disable_adc_high_speed_mode() (ADCSRB &= ~(1<<ADHSM))

## Detailed Description

Set the high spped mode in case ADC frequency is higher than 200KHz.

## Define Documentation

#define Enable_adc_high_speed_mode | ( |  | ) | (ADCSRB |= (1<<ADHSM))

Definition at line 75 of file adc_drv.h.

#define Disable_adc_high_speed_mode | ( |  | ) | (ADCSRB &= ~(1<<ADHSM))

Definition at line 76 of file adc_drv.h.