ATMEL: usb_device_task.h File Reference

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# usb_device_task.h File Reference

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Defines

#define | B_IDLE 0
#define | B_SRP_INIT 1
#define | B_PERIPHERAL 2
#define | B_WAIT_ACON 3
#define | B_HOST 4
#define | B_END_HNP_SUSPEND 5
#define | Start_session_with_srp() (otg_device_sessions |= 0x01)
| Is the current session a result of a SRP ?
#define | End_session_with_srp() (otg_device_sessions &= ~0x01)
#define | Is_session_started_with_srp() (((otg_device_sessions&0x01) != 0) ? TRUE : FALSE)
#define | Srp_sent_and_waiting_answer() (otg_device_sessions |= 0x02)
| Has a SRP been sent, and waiting for an answer.
#define | Ack_srp_sent_and_answer() (otg_device_sessions &= ~0x02)
#define | Is_srp_sent_and_waiting_answer() (((otg_device_sessions&0x02) != 0) ? TRUE : FALSE)
#define | TB_SRP_FAIL_MIN 0x0A28
| Is the Tb_Srp counter enabled ? Cleared by timer if Tb_Srp_Fail elapsed.
#define | Init_tb_srp_counter() (otg_tb_srp_cpt = 0)
#define | Is_tb_srp_counter_overflow() ((otg_tb_srp_cpt > TB_SRP_FAIL_MIN) ? TRUE : FALSE)

## Functions

void | usb_device_task_init (void)
void | usb_start_device (void)
void | usb_device_task (void)

## Variables

bit | usb_suspended
| Public : (bit) usb_suspended usb_suspended is set to TRUE when USB is in suspend mode usb_suspended is set to FALSE otherwise /.
U8 | otg_device_sessions
| Public : (U8) otg_device_sessions; Store some events and conditions specifics to OTG Devices sessions.
U8 | otg_b_device_state
| Public : (U8) otg_b_device_state; Store the current state of the B-Device.
U8 | sof_seen_in_session
| Public : (U8) sof_seen_in_session; Indicates if a SOF has been received during the current session /.
U16 | otg_tb_srp_cpt
| Public : (U16) otg_tb_srp_cpt; Counter used to signal a SRP fail condition (SRP fails if Tb_Srp_Fail elapsed).

## Detailed Description

This file contains the function declarations for USB device task - Compiler: IAR EWAVR and GNU GCC for AVR

- Supported devices: AT90USB1287, AT90USB1286, AT90USB647, AT90USB646
  Author:
    Atmel Corporation: http://www.atmel.com
    Support and FAQ: http://support.atmel.no/

Definition in file usb_device_task.h.