ATMEL: ADC Start Idle Conversion

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# ADC Start Idle Conversion
[ADC Start Conversion]

Start the Analog to Digital Conversion in noise reduction mode. More...

## Defines

#define | Start_conv_idle() (SMCR |= (1<<SM0)|(1<<SE) )
#define | Start_conv_idle_channel(channel) (Select_adc_channel(channel), Start_conv_idle() )
#define | Clear_sleep_mode() (SMCR &= ~(1<<SM0)|(1<<SE) )

## Detailed Description

Start the Analog to Digital Conversion in noise reduction mode.

## Define Documentation

#define Start_conv_idle | ( |  | ) | (SMCR |= (1<<SM0)|(1<<SE) )

Definition at line 130 of file adc_drv.h.

#define Start_conv_idle_channel | ( | channel |  | ) | (Select_adc_channel(channel), Start_conv_idle() )

Definition at line 131 of file adc_drv.h.

#define Clear_sleep_mode | ( |  | ) | (SMCR &= ~(1<<SM0)|(1<<SE) )

Definition at line 132 of file adc_drv.h.