ATMEL: power_drv.h File Reference

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# power_drv.h File Reference

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Defines

#define | Setup_idle_mode() (SMCR=0,SMCR |= (1<<SE))
#define | Setup_power_down_mode() (SMCR=0,SMCR |= (1<<SE)+(1<<SM1))
#define | Setup_adc_noise_reduction_mode() (SMCR=0,SMCR |= (1<<SE)+(1<<SM0))
#define | Setup_power_save_mode() (SMCR=0,SMCR |= (1<<SE)+(1<<SM1)+(1<<SM0))
#define | Setup_standby_mode() (SMCR=0,SMCR |= (1<<SE)+(1<<SM2)+(1<<SM1))
#define | Setup_ext_standby_mode() (SMCR=0,SMCR |= (1<<SE)+(1<<SM2)+(1<<SM1)+(1<<SM0))
#define | Clear_prescaler() (Set_cpu_prescaler(0))
| This function reset the internal CPU core clock prescaler.
#define | Sleep_instruction() {asm("SLEEP");}
#define | Set_power_down_mode() set_power_down_mode()
#define | Set_idle_mode() set_idle_mode()
#define | Enter_idle_mode() (set_idle_mode())
| This function makes the AVR core enter idle mode.
#define | Enter_power_down_mode() (set_power_down_mode())
| This function makes the AVR core enter power down mode.
#define | Enter_adc_noise_reduction_mode() (set_adc_noise_reduction_mode())
| This function makes the AVR core enter adc noise reduction mode.
#define | Enter_power_save_mode() (set_power_save_mode())
| This function makes the AVR core enter power save mode.
#define | Enter_standby_mode() (set_standby_mode())
| This function makes the AVR core enter standby mode.
#define | Enter_ext_standby_mode() (set_ext_standby_mode())
| This function makes the AVR core enter extended standby mode.

## Functions

void | Set_cpu_prescaler (U8 x)
| This function configure the internal CPU core clock prescaler value.
void | set_idle_mode (void)
| This function makes the AVR core enter idle mode.
void | set_power_down_mode (void)
| This function makes the AVR core enter power down mode.
void | set_adc_noise_reduction_mode (void)
| This function makes the AVR core enter adc noise reduction mode.
void | set_power_save_mode (void)
| This function makes the AVR core enter power save mode.
void | set_standby_mode (void)
| This function makes the AVR core enter standby mode.
void | set_ext_standby_mode (void)
| This function makes the AVR core enter extended standby mode.

## Detailed Description

This file contains the Power Management low level driver definition This module allows to configure the different power mode of the AVR core and also to setup the the internal clock prescaler - Compiler: IAR EWAVR and GNU GCC for AVR

- Supported devices: AT90USB1287, AT90USB1286, AT90USB647, AT90USB646
  Author:
    Atmel Corporation: http://www.atmel.com
    Support and FAQ: http://support.atmel.no/

Definition in file power_drv.h.