ATMEL: Fs_file_segment Struct Reference

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Alphabetical List
- Data Structures
- Data Fields

# Fs_file_segment Struct Reference

`#include <file.h>`

## Data Fields

U8 | u8_lun
| logical unit(drive) number
U32 | u32_addr
| segment address (unit sector)
U16 | u16_size
| segment size (unit sector), or IN parameter for file_write() and file_read() routines

## Detailed Description

Definition at line 62 of file file.h.

## Field Documentation

U8 Fs_file_segment::u8_lun

logical unit(drive) number

Definition at line 63 of file file.h.

Referenced by ushell_cmd_perform_access(), ushell_cmd_perform_extaccess(), and ushell_cmd_perform_transfer().

U32 Fs_file_segment::u32_addr

segment address (unit sector)

Definition at line 64 of file file.h.

Referenced by ushell_cmd_perform_access(), ushell_cmd_perform_extaccess(), and ushell_cmd_perform_transfer().

U16 Fs_file_segment::u16_size

segment size (unit sector), or IN parameter for file_write() and file_read() routines

Definition at line 65 of file file.h.

Referenced by ushell_cmd_perform(), ushell_cmd_perform_access(), ushell_cmd_perform_alloc(), ushell_cmd_perform_extaccess(), and ushell_cmd_perform_transfer().

The documentation for this struct was generated from the following file:

- file.h