ATMEL: config.h Source File

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# config.h

Go to the documentation of this file.

    00001 /*This file is prepared for Doxygen automatic documentation generation.*/
    00013
    00014 /* Copyright (c) 2009 Atmel Corporation. All rights reserved.
    00015  *
    00016  * Redistribution and use in source and binary forms, with or without
    00017  * modification, are permitted provided that the following conditions are met:
    00018  *
    00019  * 1. Redistributions of source code must retain the above copyright notice,
    00020  * this list of conditions and the following disclaimer.
    00021  *
    00022  * 2. Redistributions in binary form must reproduce the above copyright notice,
    00023  * this list of conditions and the following disclaimer in the documentation
    00024  * and/or other materials provided with the distribution.
    00025  *
    00026  * 3. The name of Atmel may not be used to endorse or promote products derived
    00027  * from this software without specific prior written permission.
    00028  *
    00029  * 4. This software may only be redistributed and used in connection with an Atmel
    00030  * AVR product.
    00031  *
    00032  * THIS SOFTWARE IS PROVIDED BY ATMEL "AS IS" AND ANY EXPRESS OR IMPLIED
    00033  * WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
    00034  * MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NON-INFRINGEMENT ARE EXPRESSLY AND
    00035  * SPECIFICALLY DISCLAIMED. IN NO EVENT SHALL ATMEL BE LIABLE FOR ANY DIRECT,
    00036  * INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
    00037  * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
    00038  * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
    00039  * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
    00040  * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF
    00041  * THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
    00042  */
    00043
    00044 #ifndef _CONFIG_H_
    00045 #define _CONFIG_H_
    00046
    00047 // Compiler switch (do not change these settings)
    00048 #include "lib_mcu/compiler.h"             // Compiler definitions
    00049 #ifdef __GNUC__
    00050    #include <avr/io.h>                    // Use AVR-GCC library
    00051 #elif __ICCAVR__
    00052    #define ENABLE_BIT_DEFINITIONS
    00053    #include <ioavr.h>                     // Use IAR-AVR library
    00054 #else
    00055    #error Current COMPILER not supported
    00056 #endif
    00057
    00058
    00061
    00062 #include "conf/conf_scheduler.h"          // Scheduler tasks declaration
    00063
    00065 #define USE_ADC
    00066
    00068 #define  STK525   1                       // do not change these settings
    00069 #define  TARGET_BOARD STK525
    00070 #include "lib_board\stk_525\stk_525.h"
    00071
    00073 #define FOSC 8000
    00074
    00075 #define USE_TIMER16 TIMER16_1
    00076
    00077 // -------- END Generic Configuration -------------------------------------
    00078
    00080 #define HID_GENERIC_DEMO_FULL   DISABLE
    00081
    00082 #define HOST_SYNC_MODE  ENABLE
    00083
    00084 // UART Sample configuration, if we have one ... __________________________
    00085 #define BAUDRATE        57600
    00086 #define USE_UART2
    00087 #define UART_U2
    00088
    00089 #ifndef __GNUC__
    00090 #define uart_putchar putchar
    00091 #endif
    00092
    00093 #define r_uart_ptchar int
    00094 #define p_uart_ptchar int
    00095
    00096
    00097 // ADC Sample configuration, if we have one ... ___________________________
    00098
    00100 #define ADC_PRESCALER 32
    00102 #define ADC_RIGHT_ADJUST_RESULT 1
    00104 #define ADC_INTERNAL_VREF  2
    00105
    00106 #define SBC_VENDOR_ID         {'A','T','M','E','L',' ',' ',' '}      // 8 Bytes only
    00107 #define SBC_PRODUCT_ID        {'A','T','9','0','U','S','B','1','2','8',' ','M',' ','S',' ',' '}  // 16 Bytes only
    00108 #define SBC_REVISION_ID       {'0','.','0','0'}  // 4 Bytes only
    00109
    00111 #define NB_IDLE_POLLING_SOF  2
    00112 #define MOUSE_SPEED          3
    00113
    00114 // Nav_util.c configuration
    00115 #define MAX_FILE_LENGHT       30
    00116
    00117 // USHELL configuration, if we have one ... ___________________________
    00118
    00119 #define USHELL_DFU            ENABLE
    00120 #define USHELL_USB            ENABLE
    00121 #define USHELL_HID            ENABLE
    00122 #define USHELL_HISTORY        5
    00123 #define USHELL_SIZE_CMD_LINE  30
    00124 #define USHELL_NB_LINE        20
    00125 #define USHELL_SIZE_OF_EXT_BUFFER_TO_PERF_CMD 4
    00126
    00127 #define TRACE                 DISABLE
    00128
    00129 #if (TRACE==ENABLE)
    00130 extern void ushell_trace_msg(U8 code *str);
    00131 #define LOG_STR_CODE(s)    ushell_trace_msg(s)
    00132 #endif
    00133
    00134
    00135
    00137
    00138 #endif // _CONFIG_H_
    00139