ATMEL: USB Pads Regulator drivers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

# USB Pads Regulator drivers
[USB low level drivers]

Turns ON/OFF USB pads regulator. More...

## Defines

#define | Usb_enable_regulator() (UHWCON |= (1<<UVREGE))
| Enable internal USB pads regulator.
#define | Usb_disable_regulator() (UHWCON &= ~(1<<UVREGE))
| Disable internal USB pads regulator.
#define | Is_usb_regulator_enabled() ((UHWCON & (1<<UVREGE)) ? TRUE : FALSE)
| Check regulator enable bit.

## Detailed Description

Turns ON/OFF USB pads regulator.

## Define Documentation

#define Usb_enable_regulator | ( |  | ) | (UHWCON |= (1<<UVREGE))

Enable internal USB pads regulator.

Definition at line 202 of file usb_drv.h.

Referenced by usb_task_init().

#define Usb_disable_regulator | ( |  | ) | (UHWCON &= ~(1<<UVREGE))

Disable internal USB pads regulator.

Definition at line 204 of file usb_drv.h.

#define Is_usb_regulator_enabled | ( |  | ) | ((UHWCON & (1<<UVREGE)) ? TRUE : FALSE)

Check regulator enable bit.

Definition at line 206 of file usb_drv.h.