digraph G
{
  edge [fontname="FreeSans.ttf",fontsize=10,labelfontname="FreeSans.ttf",labelfontsize=10];
  node [fontname="FreeSans.ttf",fontsize=10,shape=record];
  rankdir=LR;
  Node1 [label="df_write_10",height=0.2,width=0.4,color="black", fillcolor="grey75", style="filled" fontcolor="black"];
  Node1 -> Node2 [color="midnightblue",fontsize=10,style="solid",fontname="FreeSans.ttf"];
  Node2 [label="df_mem_init",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$a00059.html#904988fe40f0fc0d9ccf9b4041e5133e",tooltip="This function initializes the hw/sw ressources required to drive the DF."];
  Node1 -> Node3 [color="midnightblue",fontsize=10,style="solid",fontname="FreeSans.ttf"];
  Node3 [label="df_write_close",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$a00057.html#0ab831b820f2a30a2e273a7e7e820252",tooltip="This function fills the end of the logical sector (512B) and launch page programming..."];
  Node1 -> Node4 [color="midnightblue",fontsize=10,style="solid",fontname="FreeSans.ttf"];
  Node4 [label="df_write_open",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$a00057.html#ff167c7f03438afd57e148a2d12ade41",tooltip="This function opens a DF memory in write mode at a given sector address."];
  Node1 -> Node5 [color="midnightblue",fontsize=10,style="solid",fontname="FreeSans.ttf"];
  Node5 [label="df_write_sector",height=0.2,width=0.4,color="black", fillcolor="white", style="filled",URL="$a00057.html#2241c23b970d692b0698dd7d75eb41b5",tooltip="This function is optimized and writes nb-sector * 512 Bytes from USB controller to..."];
}
